**Performance Based Specifications**

**Wall Surface Mounted, ADA, High Efficiency, Heated, eHEPA, Electric Hand Dryer**

**Performance Requirements**

* Dry Time: 14 seconds or less - PCR Tested (Product Category Rules) for Hand Dryers
* Environmental Product Declarations: Product EPD per ISO 14044
* Air Velocity: 11,000 - 18,000 LFM @ Air Outlet
* Flow Rate: 27 - 44 CFM
* Motor RPM: Up to 31,000 RPM
* Voltage: Available in both low-voltage (110V/120V) or high voltage (208V to 277V)
* Wattage: 950 Watts
* Energy Per Use: 3.7 Wh
* Depth of the cover not to exceed 3 15/16”
* Adjustable Speed & Sound Control
* Adjustable Heat Control– High, Medium, Low, Off
* Externally Visible Service LED
* Electrostatic HEPA (eHEPA) Filtration
* Washable metal mesh prefilter
* Mounting: Wall mounted
* Finish: As selected from manufacturer’s standard options
* 5 Year Warranty
* Made in the USA Certified

**Approved Manufactures**

* Excel Dryer
* Sloan Valve Company
* Liberty Enterprises