**Performance Based Specifications**

**Wall Mounted, High-Speed, Energy Efficient, No Heat, eHEPA, Electric Hand Dryer**

**Performance Requirements**

* Dry Time: 10 seconds or less - PCR Tested (Product Category Rules) for Hand Dryers
* Environmental Product Declarations: Product EPD per ISO 14044
* Air Velocity: 13,000 - 20,000 LFM @ Air Outlet
* Flow Rate: 43 - 65 CFM
* Motor RPM: Up to 24,000 RPM
* Voltage: Available in both low-voltage (110V/120V) or high voltage (208V to 277V)
* Wattage: 500 Watts
* Energy Per Use: 1.7 Wh
* Adjustable Speed & Sound Control
* Externally Visible Service LED
* Electrostatic HEPA (eHEPA) Filtration
* Washable metal mesh prefilter
* Mounting/ADA: Wall mounted, ADA compliant with recess kit
* Finish: As selected from manufacturer’s standard options
* 7 Year Warranty
* Made in the USA Certified

**Approved Manufactures**

* Excel Dryer
* Sloan Valve Company
* Liberty Enterprises